*Release note*

1. Version 6.0 – ( 11/11/18)
   1. Graphical change
   2. Modbus write command support
   3. Save Modbus read response in CVS format
   4. Access (Read and Write) device by individual or selected scanned or all scanned device
   5. Both Modbus read and write supported from .xls file and value from txt box – Write Modbus command implementation incomplete
   6. Restore with configuration compatibly